Ingenico (Download INGEMV3) (Ethernet)

**Option A**

1. **Press F Key**
2. **Type in password 1234562, F, then Enter (F is to change 2 to the letter A)**
3. **Select Telium Manager (might ask for default password)**
4. **Select Initialization**
5. **Select Hardware**
6. **Select Ethernet Setup**
7. **Select Boot Proto**
8. **Select either DHCP (Dynamic IP) or Static Address**

**\*\*\* If Static address, you will need to enter IP address, Subnet Mask, Gateway and DNS1 \*\*\***

1. **Scroll to Quit**
2. **Terminal should prompt to Save, select yes**
3. **Terminal should restart**

**Option B**

1. **Press F Key**
2. **Type in password 1234562, F, then Enter (F is to change 2 to the letter A)**
3. **Select Telium Manager**
4. **Select Initialization**
5. **Select Parameters**
6. **Select T.M.S (must scroll down to this option)**
7. **Select IP/Eth (must scroll down to this option)**
8. **Screen displays SSL-PKIV1 or SSL-PKIV3, select yes**
9. **Screen displays Profile SSL-PKIV1, select TADU\_SSL**
10. **Select IP address instead of Domain name**
11. **Screen displays IP Address, Select IP address 209.154.100.063 (Use # for period in between numbers)**
12. **Select Doman Name: download.tsysacquiring.net**
13. **NOTE: Do not use F key to change numbers to letters, If you want letter A, just press number 2 two times then enter**

* **Screen displays PORT\_PKIV1, type in 32605**
* **Screen displays TMS Identifier, Terminal id #’s should already there (type in terminal id with 7 replacing the V)**
* **Screen displays Protect download, select offScreen displays Remote Unprotected, press cancel twice until you get back to the TSYS screen**

**Option B**

1. **Press F Key**
2. **Type in password 1234562, F, then enter**

**(F key is to change the number 2 to the letter A)**

1. **Select Telium Manager**
2. **Select Evolution**
3. **Select Remote Load**
4. **On the “Software” screen, press Enter**
   1. **Terminal will start downloading, when it connects properly, the terminal will display a percentage sign.**
5. **\*\*If terminal displays NO parameters you can retry Step 3 again. Terminal will retry download again at midnight. If it failed midnight again then terminal needs to be replace. Older software could have older version of TLS/Cipher**
6. **Once download completed you will require to authenticate terminal before process any transaction**
7. **Main Screen (TSYS or Name of business)**
8. **Press #, Press 4, Press 4, terminal will prompt for authentication code**
9. **Press 7 then F key (bottom left) 3 time it changes to S**
10. **Press 2 then F key it changes to A**
11. **Press 4 then F key it changes to G**
12. **Press 3 then F key twice it changes to E**
13. **Then enter 123 it will display SAGE123 > Press Enter**
14. **Then Enter business zip code > Enter**
15. **Terminal will display ACTIVATED**